|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| JOB/TASK NAME: Mouse Dropping Removal | | | | PAGE 1 OF 1 | | DATE: 2/17/15 | √NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB: HVAC | | | | SUPERVISOR(S): | | ANALYSIS BY: Ryan Glazier | |
| PLANT/LOCATION: HVAC | | DEPARTMENT(S): Facilities | | SHIFT (if applicable): | | APPROVED BY: | |
| PERSONAL PROTECTIVE EQUIPMENT: Goggles, Gloves, Coveralls | | | | | | | |
| TRAINING REQUIREMENTS: | | | | | | | |
| JOB STEPS | | | POTENTIAL HAZARDS | | ACTION/PROCEDURE TO CONTROL OR ELIMINATE | | |
| 1 | Section off area. Put on protective equipment. | | Slip or trip hazards | | Wear non slip safety shoes, Hepa ploo respirator, googles, gloves, protective coveralls. | | |
| 2 | Mix disinfectant solution. (1:10 bleach/water) in spray bottle, label contents of spray bottle. | | Splash hazard | | Use a funnel to pour bleach, clean up any spills. | | |
| 3 | Spray droppings gently with bleach solution, make sure they are completely soaked. Allow to sit for 15 minutes. | | Toxic dust, infectious waste, blood borne pathogens. | | Wear PPE, 15 minute soak with 10% bleach to destroy viruses. | | |
| 4 | Remove soaked material using gloves, vacuum leftover materials with a hepa filter vacuum cleaner. | | Toxic dust, infectious waste blood borne pathogens | | Wear PPE | | |
| 5 | Using 2 trash bags, place material into bag 1 and tie shut. While still wearing gloves, remove goggles, mask and protective clothing and place into bag 2, seal bag and dispose | | Toxic dust, infectious waste | | Wear PPE, Follow procedure established in step 5. | | |



Job Safety Analysis Form