|  |  |  |  |
| --- | --- | --- | --- |
| JOB/TASK NAME: Chemical Spraying | PAGE 1 OF 1 | DATE: 3/24/2015 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB: Supervising Area Supervisors | SUPERVISOR(S): Paul Snyder | ANALYSIS BY: Paul Snyder |
| PLANT/LOCATION: Outside | DEPARTMENT(S): Grounds | SHIFT (if applicable): | APPROVED BY: Chris Gale |
| PERSONAL PROTECTIVE EQUIPMENT: Long Sleeve Shirt, Pants, Non Absorbent Gloves, and Shoes |
| TRAINING REQUIREMENTS: By FEDERAL LAW the Pesticide Label is the LAW! |
| JOB STEPS | POTENTIAL HAZARDS | ACTION/PROCEDURE TO CONTROL OR ELIMINATE |
| 1 | Make sure your proper personal protective clothing in on including eye protection |  | If not wearing PPE, use supplied Tyvek suits, and eye protection |
| 2 | Fill sprayer ½ of desired amount of total water | Splashing | Make sure PPE, including eye protection is being worn |
| 3 | Add chemical slowly to avoid spills or splashes | Spills, or Splashes | Same as above |
| 4 | Add remaining water | Spills, or Splashing | Same as above |
| 5 | Agitate sprayer to make sure chemical is totally mixed | Spills, or Splashing | Same as above |



Job Safety Analysis Form