|  |  |  |  |
| --- | --- | --- | --- |
| JOB/TASK NAME: Removing Outdoor Benches | PAGE 1 OF 1 | DATE: 11/4/14 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB: Kurt Higbee | SUPERVISOR(S):  | ANALYSIS BY: Kurt Higbee |
| PLANT/LOCATION: North Sacred Grove | DEPARTMENT(S): Grounds | SHIFT (if applicable): | APPROVED BY: Chris Gale |
| PERSONAL PROTECTIVE EQUIPMENT: Leather Gloves, Safety Glasses, Dust Mask, Earplugs  |
| TRAINING REQUIREMENTS:  |
| JOB STEPS | POTENTIAL HAZARDS | ACTION/PROCEDURE TO CONTROL OR ELIMINATE |
| 1 | Rake soil away from bench posts | Step on rake head | Lean it up and move away from project, or load in cart |
| 2 | Use sawzall to cut posts | Metal and wood chips in eyes | PPE safety glasses, dust mask, ear plugs |
| 3 | Switch blades cut wood in between posts | Wood and metal particles in air | PPE dust mask |
| 4 | Load cut pieces on cart to haul away to the trash | Wood and metal slivers in hands | PPE Leather gloves |
| 5 |  |  |  |



Job Safety Analysis Form